Discussion:

The tsfc decreases when the Overall Pressure Ratio increases and the Turbine Inlet Temperature decreases. According to the tsfc vs Fs plot there is a more linear relationship between Fs and tsfc for lower OPR values and a more curvilinear relationship between Fs and tsfc for higher OPR values. The parabolic profile for constant Turbine inlet temperatures are more spread out for lower TINT values.